Greaseweazle Commands:

write IMD to DS/DD 5.25 Floppy:

gw write images\S-100\SBC548N_vector_ZCB_serialA_04_05.IMD --drive B --tracks="c=0-34:step=2" --dd L
gw write images\S-100\SBC548N_spdtabB8_step0.IMD --drive B --tracks="c=0-34:step=2" --dd L
